**Item No. Description Quantity Unit Total**

**2 WOOD-ALUMINIUM CONSTRUCTIONS**

**2.4 Exterior Window Cills**

2.4.1 Exterior Window Cill

in light metal in conformity with the system description and previous notices with underside noise suppression coating to be mounted to the building in diverse individual lengths and specified window elements, incl. fixing materials, connecting profiles, and corner joints.

Profile: 4-times folded, upper screw surface and lower drip edge

Material: Aluminium

Outreach: 300 mm, Protrusion: 40 mm

Side connection: According to specific position

Colour: same colour as for wood-aluminium elements or RAL at the choice of the Principal

174 m ........................... ..............................

2.4.2 Window Cill Pieces

as driving rain-resistant sliding end piece for the specified profiles to be supplied and mounted to the exterior window cills.

286 pieces ........................... ..............................